Hanger Door Operation
The doors on the Seaplane Terminal hanger and the DC-4 hanger open and close in response to setting frequencies on the Nav 2 radio as follows:
	Seaplane hanger: set Nav 2 to 112.00
	DC-4 Ops hanger:  set Nav 2 to 113.00
Wait 10-15 seconds and the doors will open.  
Doors are closed by setting Nav 2 to any other frequency.  
There are small signs on each hanger identifying the frequency for operating the doors.
